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CEOS-ARD - Synthetic Aperture Radar - Ocean Radar Backscatter
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CEOS Analysis Ready Data Definition
CEOS Analysis Ready Data (CEOS-ARD) are satellite data that have been processed to a minimum set of requirements and organized into a form that allows immediate analysis with a minimum of additional user effort and interoperability both through time and with other datasets.
Description
Product Family Specification: Synthetic Aperture Radar, Ocean Radar Backscatter (ORB)
Version: 1.1.0-draft
Applies to: Data collected by Synthetic Aperture Radar sensors
Background
This PFS is specifically aimed at users interested in exploring the potential of SAR but who may lack the expertise or facilities for SAR processing.
The CEOS-ARD Ocean Radar Backscatter (ORB) product specification describes products that have been projected on a geoid and are provided in the Sigma-Nought () backscatter convention, which is recommended for most ocean applications. Backscatter may be calibrated to the ellipsoid () or radiometrically terrain corrected () prior to geometric terrain correction. As the basic ORB product contains backscatter values only, it cannot be directly used for SAR polarimetry or interferometric applications that require local phase estimates. Nonetheless, an advanced ORB product could include the upper diagonal of the polarimetric  covariance matrix for enabling advanced polarimetric analysis (similar to the POL product).


Definitions and Abbreviations
ACDD
Attribute Convention for Data Discovery as defined by Earth Science Information Partners (ESIP)
ALE
Absolute Geolocation Error
ATBD
Algorithm Theoretical Basis Document
Auxiliary Data
The data required for instrument processing, which does not originate in the instrument itself or from the satellite. Some auxiliary data will be generated in the ground segment, whilst other data will be provided from external sources, e.g., DEM, aerosols.
CB
Composite Backscatter
CEOS-ARD
Committee on Earth Observation Satellites - Analysis Ready Data
Composite Product
Product where samples (or pixels) are generated from more than one input data source, e.g. by local resolution weighting or by backscatter averaging.
CRS
Coordinate Reference System
DEM
Digital Elevation Model
DOI
Digital Object Identifier
DSM
Digital Surface Model
EGM
Earth Gravitational Model
ENL
Equivalent Number of Looks
EPSG Code
An EPSG code is a unique identifier assigned to e.g. a specific coordinate reference system (CRS) by the European Petroleum Survey Group (EPSG).
GSLC
Geocoded Single-Look Complex
ISLR
Intensity Signal-to-Noise Level Ratio
LUT
Look-Up Table
Mosaic Product
Product generated from more than one input data source and where a pixel value in the product uniquely corresponds to the pixel value of one of its input data sources.
NRB
Normalised Radar Backscatter
ORB
Ocean Radar Backscatter
PFS
Product Family Specification
POL
Polarimetric Radar
PSLR
Polarimetric Signal-to-Noise Level Ratio
rRMSE
Radial Root Mean Square Error
RTC
Radiometrically Terrain Corrected
SAR
Synthetic Aperture Radar
SI
International System of Units, internationally known by the abbreviation SI (from French Système international d’unités)
SLC
Single-Look Complex
STAC
SpatioTemporal Asset Catalog
UPS
Universal Polar Stereographic
URL
Uniform Resource Locator, a reference to a web resource that specifies its location on a computer network and a mechanism for retrieving it.
UTC
Coordinated Universal Time
UTM
Universal Transverse Mercator
WGS84
World Geodetic System 1984
WKT
Well-Known Text (WKT) is a text markup language for representing vector geometry objects on a map, spatial reference systems of spatial objects, and transformations between spatial reference systems. The formats were originally defined by the Open Geospatial Consortium (OGC) and described in their Simple Feature Access and Coordinate Transformation Service specifications.


Requirements
WARNING: The section numbers in front of the title (e.g. 1.1) are not stable and may change or may be removed at any time. Do not use the numbers to refer back to specific requirements! Instead, use the textual identifier that is provided below the title.
1. General Metadata
These are metadata records describing a distributed collection of pixels. The collection of pixels referred to must be contiguous in space and time. General metadata should allow the user to assess the overall suitability of the dataset, and must meet the requirements listed below.
1.1. Traceability
Identifier: meta-trace-sar
Threshold requirements:
Not required. 
Goal requirements:
Data must be traceable to SI reference standard.
Notes:
1. Relationship to Radiometrically Corrected Measurements: Radiometric Accuracy. Traceability requires an estimate of measurement uncertainty.
1. Information on traceability should be available in the metadata as a single DOI landing page.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

1.2. Metadata Machine Readability
Identifier: meta-memare-sar
Threshold requirements:
Metadata is provided in a structure that enables a computer algorithm to be used to consistently and automatically identify and extract each component/variable for further use.
Goal requirements:
As threshold, but metadata is formatted in accordance with the latest corresponding CEOS-ARD SAR Metadata Specifications, or in a community endorsed standard that facilitates machine-readability, such as ISO 19115-2, Climate and Forecast (CF) convention and the Attribute Convention for Data Discovery (ACDD), etc.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

1.3. Product Type
Identifier: meta-protype
Threshold requirements:
CEOS-ARD product type name – or names in case of compliance with more than one product type – and, if required by the data provider, copyright.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

1.4. Document Identifier
Identifier: meta-pfsurl
Threshold requirements:
Reference to CEOS-ARD PFS document as URL.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

1.5. Data Collection Time
Identifier: meta-time-sar
Threshold requirements:
Number of source data acquisitions of the data collection is identified. The start and stop UTC time of data collection is identified in the metadata, expressed in date/time. In the case of composite or mosaic products, the dates/times of the first and last data takes is provided with the product.
Goal requirements:
As threshold, but using ISO 8601 time format.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:
2. Source Metadata
Metadata describing (detailing) each acquisition used to generate the ARD product.
Source data attribute information can refer to other products for higher level ARD derived from those, under the condition of their availability (Source Metadata: Source Data Access).
2.1. Acquisition ID
Identifier: src-macqid
Threshold requirements:
Source data attribute information are described for each acquisition and sequentially identified e.g. as acqID = 1, 2, 3, …
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.2. Source Data Access
Identifier: src-daccess-src
Threshold requirements:
The metadata identifies the location from where the source data can be retrieved, expressed as a URL or DOI.
Goal requirements:
The metadata identifies an online location from where the data can be consistently and reliably retrieved by a computer algorithm without any manual intervention being required.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.3. Instrument
Identifier: src-instru-sar
Threshold requirements:
The instrument used to collect the data is identified in the metadata:
· Satellite name
· Instrument name
Goal requirements:
As threshold, but using CEOS Mission-Instruments-Measurements (MIM) database as reference.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.4. Source Data Acquisition Time
Identifier: src-time-src
Threshold requirements:
The start date and time of source data is identified in the metadata, expressed in UTC in date and time, at least to the second.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.5. Source Data Acquisition Parameters
Identifier: src-acqpar
Threshold requirements:
Acquisition parameters related to the SAR antenna:
· Radar band
· Centre frequency
· Observation mode (i.e., beam mode name)
· Polarization(s) (listed as in original product)
· Antenna pointing (right/left)
· Beam ID (i.e., beam mode mnemonic)
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.6. Source Data Orbit Information
Identifier: src-orbit
Threshold requirements:
Information related to the platform orbit used for data processing:
· Pass direction (asc/desc), see note
· Orbit data source (e.g., predicted, definite, precise, downlinked, etc.)
Note:
1. For source data crossing the North or South Pole, it is recommended to produce two distinct CEOS-ARD products and to use the appropriate “Pass direction” in each.
Goal requirements:
As threshold, including also:
· Platform heading angle expressed in degrees (0-360) from North
· Orbit data file containing state vectors (minimum of 5 state vectors, from 10% of scene length before start time to 10% of scene length after stop time)
· Platform (mean) altitude
· Absolute orbit number
· Relative orbit number
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.7. Source Data Processing Parameters
Identifier: src-propar
Threshold requirements:
Processing parameters details of the source data:
· Processing facility
· Processing date
· Software version
· Product level
· Product ID (file name)
· Azimuth number of looks
· Range number of looks (separate values for each beam, as necessary)
Note:
1. Azimuth and Range number of looks are not required when sources are CEOS-ARD or any other geocoded products
Goal requirements:
As threshold, plus additional relevant processing parameters, e.g., range- and azimuth look bandwidth and LUT applied.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.8. Source Data Image Attributes
Identifier: src-imgatt-sar
Threshold requirements:
Image attributes related to the source data:
· Source data geometry (slant range/ground range/geocoded)
· Azimuth pixel spacing [m] (alternatively, azimuth pixel spacing can be provided in second [s], equivalent to the azimuth time sample interval)
· Range pixel spacing
· Azimuth resolution
· Range resolution
· Near range incident angle
· Far range incident angle
Note:
1. For geocoded sources such as GSLC and InSAR, Azimuth and Range pixel spacing are replaced by line (row) and pixel (column) spacing information. Spatial resolution information is not required for geocoded sources.
Goal requirements:
Geometry of the image footprint expressed in WGS84 in a standardised format (e.g., WKT).
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.9. Sensor Calibration
Identifier: src-sencal-sar
Threshold requirements:
Not required. 
Goal requirements:
Sensor calibration parameters are identified in the metadata or can be accessed using details included in the metadata. Ideally this would support machine-to-machine access.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.10. Performance Indicators
Identifier: src-perfind
Threshold requirements:
Provide performance indicators on data intensity noise level ( and/or  and/or , i.e., noise equivalent Sigma- and/or Beta- and/or Gamma-Nought). Provided for each polarization channel when available.
Parameter may be expressed as the mean and/or minimum and maximum noise equivalent values of the source data.
Values do not need to be estimated individually for each product, but may be estimated once for each acquisition mode, and annotated on all products.
Goal requirements:
Provide additional relevant performance indicators (e.g., ENL, PSLR, ISLR, and performance reference DOI or URL).
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.11. Polarimetric Calibration Matrices
Identifier: src-polcalm
Threshold requirements:
Not required. 
Goal requirements:
The complex-valued polarimetric distortion matrices with the channel imbalance and the cross-talk applied for the polarimetric calibration.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.12. Mean Faraday Rotation Angle
Identifier: src-farotan
Threshold requirements:
Not required. 
Goal requirements:
The mean Faraday rotation angle estimated from the polarimetric data and/or from models with reference to the method or paper used to derive the estimate.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

2.13. Ionosphere Indicator
Identifier: src-ionind
Threshold requirements:
Not required. 
Goal requirements:
Flag indicating whether the backscatter imagery is “significantly impacted” by the ionosphere (0 – false, 1 – true). Significant impact would imply that the ionospheric impact on the backscatter exceeds the radiometric calibration requirement or goal for the imagery.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:
3. Product Metadata
Information related to the CEOS-ARD product generation procedure and geographic parameters.
3.1. Product Data Access
Identifier: prd-daccess-prod
Threshold requirements:
Processing parameters details of the CEOS-ARD product:
· Processing facility
· Processing date
· Software version
· Location from where CEOS-ARD product can be retrieved, expressed as a URL or DOI.
Goal requirements:
The metadata identifies an online location from where the data can be consistently and reliably retrieved by a computer algorithm without any manual intervention being required.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.2. Auxiliary Data
Identifier: prd-auxdat-sar
Threshold requirements:
Not required. 
Goal requirements:
The metadata identifies the sources of auxiliary data used in the generation process, ideally expressed as DOIs.
Note:
1. Auxiliary data includes DEMs, etc., and any additional data sources used in the generation of the product.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.3. Product Sample Spacing
Identifier: prd-samspa
Threshold requirements:
CEOS-ARD product processing parameters details:
· Pixel (column) spacing
· Line (row) spacing
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.4. Product Equivalent Number of Looks
Identifier: prd-enl
Threshold requirements:
Not required. 
Goal requirements:
Equivalent Number of Looks (ENL)
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.5. Product Resolution
Identifier: prd-resol
Threshold requirements:
Not required. 
Goal requirements:
Average spatial resolution of the CEOS-ARD product along:
· Columns
· Rows
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.6. Product Filtering
Identifier: prd-spekfil
Threshold requirements:
Flag if speckle filter has been applied (true/false).
Metadata should include:
· Reference to algorithm as DOI or URL
· Input filtering parameters
· Type
· Window size in pixel units
· Any other parameters defining the speckle filter used
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.7. Product Bounding Box
Identifier: prd-geobbox
Threshold requirements:
Two opposite corners of the product file (bounding box, including any zero-fill values) are identified, expressed in the coordinate reference system defined in Product Metadata: Product Coordinate Reference System.
Four corners of the product file are recommended for scenes crossing the Antemeridian, or the North or the South Pole.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.8. Product Geographical Extent
Identifier: prd-geoarea-sar
Threshold requirements:
The geometry of the SAR image footprint expressed in longitude/latitude based on WGS84 (EPSG 4326), in a standardised format (e.g., WKT Polygon).
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.9. Product Image Size
Identifier: prd-imgsize
Threshold requirements:
Image attributes of the CEOS-ARD product:
· Number of lines
· Number of pixels per line
· File header size (if applicable)
· Number of no-data border pixels (if applicable)
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.10. Product Pixel Coordinate Convention
Identifier: prd-pixcoco
Threshold requirements:
Coordinate referring to the centre, the upper left corner, or the lower left corner of a pixel. Values are pixel centre, pixel ULC or pixel LLC.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.11. Product Coordinate Reference System
Identifier: prd-crs-sar
Threshold requirements:
The metadata lists the map projection (or geographical coordinates, if applicable) that was used and any relevant parameters required to geolocate data in that map projection, expressed in a standardised format (e.g., WKT).
Indicate EPSG code, if defined for the CRS.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

3.12. Look Direction Polynomials
Identifier: prd-lookdip
Threshold requirements:
In case the Look Direction Image (see Per-Pixel Metadata: Look Direction Image) is not provided, then a list of the polynomial coefficients are necessary to reconstruct the look direction angle[footnoteRef:157], together with an estimate of the added error from use of polynomial vs. per-pixel more accurate values, shall be provided. [157:  The look direction angle represents the planar angle between north and each range direction. It is not constant in range, especially close to the poles.] 

Example polynomial:

where:
·  = polynomial coefficients
·  = latitude

·  = longitude
Lat and Lon are the related coordinates in the product map units (m, deg, arcsec).
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:
4. Per-Pixel Metadata
The following minimum metadata specifications apply to each pixel. Whether the metadata is provided in a single record relevant to all pixels or separately for each pixel is at the discretion of the data provider. Per-pixel metadata should allow users to discriminate between (choose) observations on the basis of their individual suitability for application.
4.1. Metadata Machine Readability
Identifier: pxl-memare-sar
Threshold requirements:
Metadata is provided in a structure that enables a computer algorithm to be used to consistently and automatically identify and extract each component/variable for further use.
Goal requirements:
As threshold, but metadata is formatted in accordance with the latest corresponding CEOS-ARD SAR Metadata Specifications, or in a community endorsed standard that facilitates machine-readability, such as ISO 19115-2, Climate and Forecast (CF) convention and the Attribute Convention for Data Discovery (ACDD), etc.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.2. Data Mask Image
Identifier: pxl-damaski
Threshold requirements:
Mask image indicating:
· Valid data
· Invalid data
· No data
File format specifications/contents provided in metadata:
· Sample Type (Mask)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, …)
· Bits per Sample
· Byte Order
· Bit Value Representation
Notes:
1. All bit value representations included in the Data Mask Image should be indicated in the metadata.
1. For CEOS-ARD products created from repeat-pass acquisitions, with narrow orbital tube radius, a single static per pixel metadata file can be provided as a URL address of that unique metadata file.
Goal requirements:
As threshold, including additional bit value representations, e.g.:
· Layover (masked as invalid data in threshold)
· Radar shadow (masked as invalid data in threshold)
· Ocean water
· Land (recommended for ORB)
· RTC applied (e.g., for maritime scenes with land samples for which RTC has been applied)
· DEM gap filling (i.e., interpolated DEM over gaps)
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.3. Scattering Area Image
Identifier: pxl-piscata
Usage: Recommended for scenes that include land areas.
Threshold requirements:
Not required. 
Goal requirements:
DEM-based scattering area image used for Gamma-Nought terrain normalisation is provided. This quantifies the local scattering area used to normalise for radiometric distortions induced by terrain to the measured  backscatter. The terrain-flattened  is best understood as  divided by the local scattering area.
File format specifications/contents provided in metadata:
· Sample Type (Scattering Area)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Notes:
1. For CEOS-ARD products created from repeat-pass acquisitions, with narrow orbital tube radius, a single static per pixel metadata file could be provided as a URL address of that unique metadata file.
1. Required for products such as NRB and POL if they are to be used as an input to production of composite backscatter (CB) when weighted averages based on the areas are used to generate composite backscatter.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.4. Local Incident Angle Image
Identifier: pxl-ploinca
Threshold requirements:
DEM-based Local Incident angle image is provided.
File format specifications/contents provided in metadata:
· Sample Type (Angle)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Notes:
1. For CEOS-ARD products created from repeat-pass acquisitions, with narrow orbital tube radius, a single static per pixel metadata file can be provided as a URL address of that unique metadata file.
1. For maritime ORB scenes when no land areas are covered, a geoid model could be used for the calculation of the local incident angle
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.5. Ellipsoidal Incident Angle Image
Identifier: pxl-pelinca
Threshold requirements:
Not required. 
Goal requirements:
Ellipsoidal incident angle is provided.
File format specifications/contents provided in metadata:
· Sample Type (Angle)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
· Reference Ellipsoid Name
Notes:
1. For CEOS-ARD products created from repeat-pass acquisitions, with narrow orbital tube radius, a single static per pixel metadata file can be provided as a URL address of that unique metadata file.
1. For maritime ORB scenes when no land areas are covered, the ellipsoidal incident angle is nearly identical to the geod based local incident angle
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.6. Noise Power Image
Identifier: pxl-pinopow
Threshold requirements:
Not required. 
Goal requirements:
Estimated Noise Equivalent  (or  or , as applicable) used for noise removal, if applied, for each channel.  and  are both based on either an ellipsoid Earth model or the local topography.
File format specifications/contents provided in metadata:
· Sample Type (Gamma-Nought, Sigma-Nought, Beta-Nought)
· Correction model type (Ellipsoid, Topography)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.7. Acquisition ID Image
Identifier: pxl-pacqidm
Usage: Required for mosaic products only.
Threshold requirements:
Acquisition ID, or acquisition date, for each pixel is identified.
In case of multi-temporal image stacks, use source acquisition ID (i.e., Source Metadata: Acquisition ID) to list contributing images.
In case of date, data represent (integer or fractional) day offset to reference observation date (in UTC). Date used as reference (“Day 0”) is provided in the metadata.
Pixels not representing a unique date or ID (e.g., pixels averaged in image overlap zones) are flagged with a pixel value referencing a date range that is provided in the metadata.
File format specifications/contents provided in metadata:
· Sample type (Day, Time, ID)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per sample
· Byte Order
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.8. Per-Pixel Geoid
Identifier: pxl-pigeoid
Threshold requirements:
Not required. 
Goal requirements:
Provide Geoid as used during the geometric and radiometric processing of the SAR data, resampled to an exact geometric match in extent and resolution with the CEOS-ARD image product.
File format specifications/contents provided in metadata:
· Sample Type (Height)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
· Ground Sampling Distance
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

4.9. Look Direction Image
Identifier: pxl-lookdiri
Threshold requirements:
Not required. 
Goal requirements:
Look Direction Image is provided. It represents the planar angle between north and each range direction.
File format specifications/contents provided in metadata:
· Sample Type (Angle)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Note:
1. For CEOS-ARD products created from repeat-pass acquisitions, with narrow orbital tube radius, a single static per pixel metadata file can be provided as a URL address of that unique metadata file.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:
5. Radiometrically Corrected Measurements
The requirements indicate the necessary outcomes and, to some degree, the minimum steps necessary to be deemed to have achieved those outcomes. Radiometric corrections must lead to normalised measurement(s) of backscatter intensity and/or decomposed polarimetric parameters. As for the per-pixel metadata, information regarding data format specification needs to be provided for each record. The requirements below must be met for all pixels/samples/observations in a collection.
5.1. Backscatter Measurements (ORB)
Identifier: rcm-backsca-orb
Threshold requirements:
Geoid-corrected Sigma-Nought backscatter coefficient () is provided for each polarization.
File format specifications/contents provided in metadata:
· Measurement Type (Sigma-Nought)
· Backscatter Expression Convention (linear amplitude, or linear power [see note])
· Polarization (HH, HV, VV, VH)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Note:
1. Transformation to the logarithm decibel scale is not required or desired as this step can be completed by the user if necessary.
Goal requirements:
Radiometrically Terrain-corrected Sigma-Nought backscatter coefficient () is provided for each polarization.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

5.2. Scaling Conversion
Identifier: rcm-scaconv
Threshold requirements:
If applicable, indicate the equation to convert pixel linear amplitude/power to logarithmic decibel scale, including, if applicable, the associated calibration (dB offset) factor, and/or the equation used to convert compressed data (int8/int16/float16) to float32.
Goal requirements:
As threshold, but use of float32.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

5.3. Noise Removal
Identifier: rcm-noiser
Threshold requirements:
Flag if noise removal (see note) has been applied (Y/N). Metadata should include the noise removal algorithm and reference to the algorithm as URL or DOI.
Note:
1. Thermal noise removal and image border noise removal to remove overall scene noise and scene edge artefacts, respectively.
Goal requirements:
As threshold. 
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

5.4. Radiometric Accuracy
Identifier: rcm-radacc-sar
Threshold requirements:
Not required. 
Goal requirements:
Uncertainty (e.g., bounds on  or ) information is provided as document referenced as URL or DOI. SI traceability is achieved.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

5.5. Mean Wind-Normalised Backscatter Measurements
Identifier: rcm-backsmwn
Usage: Only for Maritime scenes.
Threshold requirements:
Not required. 
Goal requirements:
Mean wind-normalised (over ocean) backscatter coefficient is provided for each available polarization. It is calculated as the ratio between the backscatter intensity and a simulated backscatter intensity image generated using an ocean surface wind model such as, e.g., (Yves et al. 1998) or (Vachon and Dobson 2000) for VV and HH polarization respectively.
File format specifications/contents provided in metadata:
· Measurement Type (Wind-Normalised Backscatter)
· Backscatter Expression Convention (intensity ratio)
· Polarization (HH, HV, VV, VH)
· Data Format (GeoTIFF, HDF5, NetCDF, …)
· Data Type (Int, Float, …)
· Bits per Sample
· Byte Order
Note:
1. Reference wind model, wind speed and direction used for reference backscattering coefficient should be provided.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:
6. Geometric Corrections
Geometric corrections are steps that are taken to place the measurement accurately on the surface of the Earth (that is, to geolocate the measurement) allowing measurements taken through time to be compared. This section specifies any geometric correction requirements that must be met in order for the data to be analysis ready.
6.1. Geometric Correction Algorithm
Identifier: gcor-geocalg
Threshold requirements:
Not required. 
Goal requirements:
Metadata references, e.g.:
· A metadata citable peer-reviewed algorithm
· Technical documentation regarding the implementation of that algorithm expressed as URLs or DOIs
· The sources of auxiliary data used to make corrections
· Resampling method used for geometric processing of the source data
Note:
1. Examples of technical documentation can include e.g., an Algorithm Theoretical Basis Document (ATBD), or a product user guide.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

6.2. Digital Elevation Model
Identifier: gcor-cdem
Usage: For products including land areas.
Threshold requirements:
1. During ortho-rectification, the data provider shall use the same DEM that was used for the radiometric terrain flattening to ensure consistency of the data stack.
1. Provide reference to the Digital Elevation Model used for geometric terrain correction. For mosaic or composite products, specify the DEM used for each input data source, if different.
1. Provide reference to Earth Gravitational Model (EGM) if used for geometric correction. For mosaic or composite products, specify the EGM used for each input data source, if different.
Goal requirements:
1. A DEM with comparable or better resolution to the resolution of the output CEOS-ARD product shall be used if available. Else, the upsampled DEM is identified.
1. Resampling method used for preparation of the DEM.
1. Method used for resampling the EGM.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

6.3. Geometric Accuracy
Identifier: gcor-geomacc-sar
Threshold requirements:
Accurate geolocation is a prerequisite to radar processing to correct for terrain and to enable interoperability between radar sensors.
The absolute geolocation error (ALE) for a sensor is typically assessed through analysis of Single Look Complex (SLC) imagery and measured along the slant range and azimuth directions (case A: SLC ALE). The end-to-end “ARD” ALE of the final CEOS-ARD product could be measured directly in the final image product in the chosen map projection, i.e., in the map coordinate directions: e.g., Northing and Easting (case B: ARD ALE). Providing accuracy estimates based on measurements following at least one scheme (A or B or both) meets the threshold requirement.
Estimates of the ALE is provided as a bias and a standard deviation, with (Case A) SLC ALE expressed in slant range and azimuth, and (Case B) ARD ALE expressed in map projection dimensions.
For composite products, when sources come from different SAR platforms or different beam modes, provide averaged ALE or averaged ARD ALE.
Notes:
1. This assessment is often made through comparison of measured corner reflector positions with their projected location in the imagery. In some cases, other mission calibration/validation results may be used.
1. The ALE is not typically assessed for every processed image, but through an ALE assessment by the data processing team characterizing all or (usually a suitably representative subset) of the generated products.
1. For new SAR missions, as long as calibration/validation reports are not available, values can be set to NaN and provide a DOI or URL link to pre-launch mission specification document.
Goal requirements:
Output product sub-sample accuracy should be less than or equal to 0.1 (slant range) pixel radial root mean square error (rRMSE).
Provide documentation of estimates of ALE as DOI or URL.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

6.4. Geometric Refined Accuracy
Identifier: gcor-georacc
Threshold requirements:
Not required. 
Goal requirements:
Values provided under Geometric Corrections: Geometric Accuracy are provided by the SAR mission Cal/Val team.
CEOS-ARD processing steps could include method refining the geometric accuracy, such as cross-correlation of the SAR data in slant range with a SAR scene simulated from a DSM or DEM.
Methodology used (name and reference), quality flag, geometric standard deviation values should be provided.
For composite products, provide averaged ALE or averaged ARD ALE estimated from all sources.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:

6.5. Gridding Convention
Identifier: gcor-gridconv
Threshold requirements:
A consistent gridding/sampling frame is used. The origin is chosen to minimise any need for subsequent resampling between multiple products (be they from the same or different providers). This is typically accomplished via a “snap to grid” in relation to the most proximate grid tile in a global system.
Note:
1. If a product hierarchy of resolutions exists (or is planned), the multiple resolutions should nest within each other (e.g., 12.5m, 25m, 50m, 100m, etc.), and not be disjoint.
Goal requirements:
Provide DOI or URL to gridding convention used.
When multiple providers share a common map projection, providers are encouraged to standardise the origins of their products among each other.
In the case of UTM/UPS coordinates, the upper left corner coordinates should be set to an integer multiple of sample intervals from a 100 km by 100 km grid tile of the Military Grid Reference System’s 100k coordinates (“snap to grid”).
For products presented in geographic coordinates (latitude and longitude), the origin should be set to an integer multiple of samples in relation to the closest integer degree.
Assessment:
· Threshold Self-Assessment:
· Goal Self-Assessment:
· Self-Assessment Explanation/ Justification:
· Recommended Requirement Modification:


Summary Self-Assessment Table
General Metadata
	Requirement ID
	Requirement Title
	Threshold
	Goal

	meta-trace-sar
	Traceability
	not required
	

	meta-memare-sar
	Metadata Machine Readability
	
	

	meta-protype
	Product Type
	
	as threshold

	meta-pfsurl
	Document Identifier
	
	as threshold

	meta-time-sar
	Data Collection Time
	
	


Source Metadata
	Requirement ID
	Requirement Title
	Threshold
	Goal

	src-macqid
	Acquisition ID
	
	as threshold

	src-daccess-src
	Source Data Access
	
	

	src-instru-sar
	Instrument
	
	

	src-time-src
	Source Data Acquisition Time
	
	as threshold

	src-acqpar
	Source Data Acquisition Parameters
	
	as threshold

	src-orbit
	Source Data Orbit Information
	
	

	src-propar
	Source Data Processing Parameters
	
	

	src-imgatt-sar
	Source Data Image Attributes
	
	

	src-sencal-sar
	Sensor Calibration
	not required
	

	src-perfind
	Performance Indicators
	
	

	src-polcalm
	Polarimetric Calibration Matrices
	not required
	

	src-farotan
	Mean Faraday Rotation Angle
	not required
	

	src-ionind
	Ionosphere Indicator
	not required
	


Product Metadata
	Requirement ID
	Requirement Title
	Threshold
	Goal

	prd-daccess-prod
	Product Data Access
	
	

	prd-auxdat-sar
	Auxiliary Data
	not required
	

	prd-samspa
	Product Sample Spacing
	
	as threshold

	prd-enl
	Product Equivalent Number of Looks
	not required
	

	prd-resol
	Product Resolution
	not required
	

	prd-spekfil
	Product Filtering
	
	as threshold

	prd-geobbox
	Product Bounding Box
	
	as threshold

	prd-geoarea-sar
	Product Geographical Extent
	
	as threshold

	prd-imgsize
	Product Image Size
	
	as threshold

	prd-pixcoco
	Product Pixel Coordinate Convention
	
	as threshold

	prd-crs-sar
	Product Coordinate Reference System
	
	as threshold

	prd-lookdip
	Look Direction Polynomials
	
	as threshold


Per-Pixel Metadata
	Requirement ID
	Requirement Title
	Threshold
	Goal

	pxl-memare-sar
	Metadata Machine Readability
	
	

	pxl-damaski
	Data Mask Image
	
	

	pxl-piscata
	Scattering Area Image
	not required
	

	pxl-ploinca
	Local Incident Angle Image
	
	as threshold

	pxl-pelinca
	Ellipsoidal Incident Angle Image
	not required
	

	pxl-pinopow
	Noise Power Image
	not required
	

	pxl-pacqidm
	Acquisition ID Image
	
	as threshold

	pxl-pigeoid
	Per-Pixel Geoid
	not required
	

	pxl-lookdiri
	Look Direction Image
	not required
	


Radiometrically Corrected Measurements
	Requirement ID
	Requirement Title
	Threshold
	Goal

	rcm-backsca-orb
	Backscatter Measurements (ORB)
	
	

	rcm-scaconv
	Scaling Conversion
	
	

	rcm-noiser
	Noise Removal
	
	as threshold

	rcm-radacc-sar
	Radiometric Accuracy
	not required
	

	rcm-backsmwn
	Mean Wind-Normalised Backscatter Measurements
	not required
	


Geometric Corrections
	Requirement ID
	Requirement Title
	Threshold
	Goal

	gcor-geocalg
	Geometric Correction Algorithm
	not required
	

	gcor-cdem
	Digital Elevation Model
	
	

	gcor-geomacc-sar
	Geometric Accuracy
	
	

	gcor-georacc
	Geometric Refined Accuracy
	not required
	

	gcor-gridconv
	Gridding Convention
	
	




Introduction
This section aims to provide background and specific information on the processing steps that can be used to achieve analysis ready data for a specific and well-developed Product Family Specification. This Guidance material does not replace or override the specifications.
What is CEOS Analysis Ready Data?
CEOS-ARD are products that have been processed to a minimum set of requirements and organized into a form that allows immediate analysis with a minimum of additional user effort. In general, these products would be resampled onto a common geometric grid (for a given product) and would provide baseline data for further interoperability both through time and with other datasets.
CEOS-ARD products are intended to be flexible and accessible products suitable for a wide range of users for a wide variety of applications, including particularly time series analysis and multi-sensor application development. They are also intended to support rapid ingestion and exploitation via high-performance computing, cloud computing and other future data architectures. They may not be suitable for all purposes and are not intended as a replacement for other types of satellite products.
When can a product be called CEOS-ARD?
The CEOS-ARD branding is applied to a particular product once:
· that product has been assessed as meeting CEOS-ARD requirements by the agency responsible for production and distribution of the product, and
· that the assessment has been peer reviewed by the relevant CEOS team(s).
Agencies or other entities considering undertaking an assessment process should consult the CEOS-ARD Governance Framework.
A product can continue to use CEOS-ARD branding as long as its generation and distribution remain consistent with the peer-reviewed assessment.
What is the difference between Threshold and Goal?
Threshold (Minimum) requirements are the minimum that is needed for the data to be analysis ready. This must be practical and accepted by the data producers.
Goal (Desired) requirements (previously referred to as “Target”) are the ideal; where we would like to be. Some providers may already meet these.
Products that meet all threshold requirements should be immediately useful for scientific analysis or decision-making.
Products that meet goal requirements will reduce the overall product uncertainties and enhance broad-scale applications. For example, the products may enhance interoperability or provide increased accuracy through additional corrections that are not reasonable at the threshold level.
Goal requirements anticipate continuous improvement of methods and evolution of community expectations, which are both normal and inevitable in a developing field. Over time, goal specifications may (and subject to due process) become accepted as threshold requirements.
Compatibility and Interoperability of CEOS-ARD SAR Products
As can be seen from the individual PFS descriptions, only a few minor details in terms of generated parameters and/or the addition of supplemental data distinguish these CEOS-ARD products. In part, they are to a large extent all backward-compatible. For example, POL products implicitly include NRB products, while a coastal NRB or POL product can simply be made compatible with other ORB products by applying gamma-to-sigma conversion. Just as GSLC can be converted to NRB (given that terrain-flattening was applied, a goal-requirement for GSLC, the inverse conversion can be made true by including the optional topographically flattened phase. In this way a NRB or POL product can be used like a GSLC for InSAR applications. Consequently, it becomes obvious that they all can follow a common approach, in terms of content and structure, in order to optimize their interoperability.
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Annexes
General Processing Roadmap
The radiometric interoperability of CEOS-ARD SAR products is ensured by a common processing chain during production. The recommended processing roadmap involves the following steps:
· Apply the best possible orbit parameters to give the most accurate product possible. These will have been projected to an ellipsoidal model such as WGS84. To achieve the level of geometric accuracy required for the DEM-based correction, precise orbit determination will be required.
· Apply instrument calibration to produce Beta-Nought values with high fidelity.
· Convert Single-Look-Complex (SLC) radiometric channel(s) to intensity NRB, ORB and POL and in addition for POL, the cross-product element(s) of the covariance as shown in annex “Normalised Covariance Matrices (CovMat)” of the applicable PFS.
· Perform radiometric terrain correction (gamma backscatter convention terrain-flattening) on the covariance matrix by applying the local surface normalisation factor to each backscatter measurement element (Small 2011; Shiroma et al. 2022).
· Perform polarimetric speckle filtering (optional for NRB and ORB), before geocoding, to optimally preserve the polarimetric information. Most popular polarimetric decomposition methodologies are incoherent in nature, which requires averaging the covariance matrix for stationarity. Depending on the application, a polarimetric filter that preserves local point targets and locally average extended targets may be used, e.g., Sigma Lee filter with 7x7 window and 3-point target (Lee et al. 2009). Multi-looking could be performed to meet optimal output sample spacing before the geometric correction step. No speckle filtering or multi-looking is performed for GSLC products.
· For GSLC products, the topographic phase is estimated relative to a reference orbit and removed from the SLC data (Zebker et al. 2010; Zebker 2017) (see annex “Topographic phase removal” in the applicable PFS)
· Geometric terrain correction (relative to geoid for ORB) is applied to the normalized backscatter measurement data. For POL, the resampling methodology should be nearest-neighbour, bilinear or average in order to preserve integrity of the covariance matrix as other resampling functions can introduce artefacts due to the mix of intensity and complex number elements in the matrix. Geocoding to a common grid structure with specified pixel spacings for true data cube format.
· Generate CEOS format metadata to accompany product layers.
· Optionally, a SpatioTemporal Asset Catalog (STAC) file is added to the product.
Table 1 lists possible sequential steps and existing software tools (e.g., Gamma software (GAMMA, 2018)) and scripting tasks that can be used to form the CEOS-ARD SAR processing roadmap.
Table 1: SAR ARD processing roadmap and software options. RADARSAT-2 Example
	Step
	Implementation option

	1. Orbital data refinement
	Check xml date and delivered format. RADARSAT-2, pre EDOT (July 2015) replace. Post July 2015, check if ‘DEF’, otherwise replace. (Gamma - RSAT2_vec)

	2. Apply radiometric scaling Look-Up Table (LUT) to Beta-Nought
	Specification of LUT on ingest.
    (Gamma - par_RSAT2_SLC/SG)

	3. Generate covariance matrix elements
	Gamma – COV_MATRIX

	4. Radiometric terrain normalisation
	Gamma - geo_radcal2

	5. Speckle filtering (Boxcar or Sigma Lee)
	Custom scripting

	6. Geometric terrain correction/Geocoding
	Gamma – gc_map and geocode_back

	7. Create metadata
	Custom scripting


Ocean Radar Backscatter example
In contrast to NRB and POL, CEOS-ARD Ocean Radar Backscatter ORB products are geoid corrected and are provided in the Sigma-Nought () backscatter convention (Figure 1), which is recommended for most ocean applications. In addition, availability of the “Local (or Ellipsoidal) Incidence Angle Image” (Figure 4) and “Look Direction Image” per-pixel metadata are highly recommended (otherwise the general metadata “Look Direction Polynomials”) since they required for operational applications like ocean wind field estimates.
The following figures show Sentinel-1 ORB products of the Tropical Cyclone Harold passing Vanuatu on April 6, 2020:
[image: assets/sar-orb-examples/S1-ORB-VV.png]
Figure 1: VV intensity; Processing: A. Rosenqvist (soloEO)
[image: assets/sar-orb-examples/S1-ORB-VH.png]
Figure 2: VH intensity; Processing: A. Rosenqvist (soloEO)
[image: assets/sar-orb-examples/S1-ORB-data-mask.png]
Figure 3: Data mask image; Processing: A. Rosenqvist (soloEO)
[image: assets/sar-orb-examples/S1-ORB-local-indicident-angle.png]
Figure 4: Local incident angle; Processing: A. Rosenqvist (soloEO)
Another useful file is the “Mean Wind-Normalised Backscatter Measurements” (Figure 6) which efficiently attenuates intensity variation along range and visually enhances oceanic features. This file is calculated as the ratio between the backscatter intensity and a simulated backscatter intensity image generated using an ocean surface wind model, like CMOD_IRF2 (Yves et al. 1998) for VV polarization or CMOD_IRF2K (Vachon and Dobson 2000) for HH polarization, and the SAR local incidence angle and the look direction information.
The following figures show Sentinel-1 EW ORB products:
[image: assets/sar-orb-examples/S1-ORB-sigma-nought.png]
Figure 5: ORB intensity (Sigma-Nought); Processing: G. Hajduch (CLS)
[image: assets/sar-orb-examples/S1-ORB-intesity-compensated.png]
Figure 6: Intensity compensated with the “Mean Wind-Normalised Backscatter Measurement” (i.e., not Sigma-Nought) and geocoded; Processing: G. Hajduch (CLS)
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